ADM. NORM for vernemasker fra 3M


4255   EN 405:2002 FFA2P3D 

ORGANISKE DAMPER : Adm.norm 5000ppm   (APF10!)

PARTIKLER: APF 20
4279  EN 405:2002 FFABEKP3D

ORGANISKE DAMPER: ADM. NORM 1000PPm (afp 10*)

SURE GASSER: ADM. NORM 1000PPm (afp 10*)

UORGANISKE GASSER: ADM. NORM 1000PPm (afp 10*)

AMMONIAKK: ADM. NORM 1000PPm (afp 10*)

PARTIKLER : APF 20
